**BATTERY SPECS**

**Voltages; 13.3**

**LVDisconnect; 9.6v**

**Capacities @ 1C rate @25°C**

**Self discharge; <1% per month**

**Peak Discharge;**

**10Ah – 500A**

**15Ah – 750A**

**23Ah – 1150A**

**zero temps – less 50%**

**Continuous Discharge; 80A**

**Std charge V; 14.4**

**Max charge V; 15.6**

**Normal charging A; up to 20A**

**Max charge A; no limit, BMS protected**

**Lifecycles; 5000@1C, 2500@10C**

**SOH life; ~ 8 yrs**

**Weight;**

**10Ah – 5.5lbs**

**15Ah – 7.1 lbs**

**23Ah – 9.9 lbs**

**Dims;**

***10 / 15Ah*;**

**7.1 x 3.2 x 6.8**

**181 x 81 x 173**

***23Ah*;**

**7.1 x 4.2 x 8.0**

**181 x 108 x 203**

**Waterproof**

**vibration resistant**

**op temps; -32 to +65 C**